1. Threshold Voltage
2. Drain current increases as is increased as increasing pulls more electrons to the surface thereby increasing the concentration of carriers which reduces the resistivity of the channel.
3. FALSE
4. is a DC values, in a MOSFET amplifier is a small AC signals.
5. Short circuit to ground

